IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2016-12-14T15:52:25"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20140223_1515(x64) - Exporter 2015.0.2014.0223 - Default UI"
Application: "Autodesk Revit 2015 (FRA)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (FRA)"

People and organizations
  Person "1411211604@qq.com" of Organization (no name given)
  Owner history of Person "1411211604@qq.com" of Organization (no name given) | application "Autodesk Revit 2015 (FRA)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (FRA)" | change NOCHANGE | created 1481680717 (2016-12-14T01:58:37Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Ductal Lafarge" | long name "Ductal Lafarge" | elevation 0.
        contains 30 elements
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Fehr® Solution Panneaux de Bardage 1,2 x 2,4 m" | object type "Basic Wall:Fehr® Solution Panneaux de Bardage 1,2 x 2,4 m:414904" | names: "Basic Wall:Fehr® Solution Panneaux de Bardage 1,2 x 2,4 m:441572" | material: layers "Basic Wall:Fehr® Solution Panneaux de Bardage 1,2 x 2,4 m" ("Fehr® panneaux standard 1.2 x 2.4m" 16., "<Unnamed>" 45., "<Unnamed>" 120., "<Unnamed>" 200.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Ductal® Solution Panneaux de Bardage 1,2 x 3,6 m" | object type "Basic Wall:Ductal® Solution Panneaux de Bardage 1,2 x 3,6 m:414954" | names: "Basic Wall:Ductal® Solution Panneaux de Bardage 1,2 x 3,6 m:441573" | material: layers "Basic Wall:Ductal® Solution Panneaux de Bardage 1,2 x 3,6 m" ("Fehr® panneaux standard 1.2 x 3.6m" 16., "<Unnamed>" 45., "<Unnamed>" 120., "<Unnamed>" 200.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Fehr® Solution Panneaux de Bardage béton/isolant" | object type "Basic Wall:Fehr® Solution Panneaux de Bardage béton/isolant:444025" | names: "Basic Wall:Fehr® Solution Panneaux de Bardage béton/isolant:443803", "Basic Wall:Fehr® Solution Panneaux de Bardage béton/isolant:621108", "Basic Wall:Fehr® Solution Panneaux de Bardage béton/isolant:621326" (+2 more) | material: layers "Basic Wall:Fehr® Solution Panneaux de Bardage béton/isolant" ("Air" 45., "Insulation" 120., "Concrete - Cast In Situ" 200.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          8 x IFCBUILDINGELEMENTPROXY | object type "Model Text:600mm Arial" | names: "Model Text:600mm Arial" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Graphics, Identity Data, Other
          7 x IFCBUILDINGELEMENTPROXY | object type "Model Text:300mm Arial" | names: "Model Text:300mm Arial" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Graphics, Identity Data, Other
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Fehr® Panneaux de Bardage 1,2 x 1,2 m" | object type "Curtain Wall:Fehr® Panneaux de Bardage 1,2 x 1,2 m:619094" | names: "Curtain Wall:Fehr® Panneaux de Bardage 1,2 x 1,2 m:618988" | parts: 123 IFCMEMBER, 70 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Horizontal Grid, Other
          2 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Fehr® Panneaux de Bardage 1,2 x 2,4 m" | object type "Curtain Wall:Fehr® Panneaux de Bardage 1,2 x 2,4 m:622402" | names: "Curtain Wall:Fehr® Panneaux de Bardage 1,2 x 2,4 m:621109", "Curtain Wall:Fehr® Panneaux de Bardage 1,2 x 2,4 m:648157" | parts: 124 IFCMEMBER, 62 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Horizontal Grid, Other
          2 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:Fehr® Panneaux de Bardage 1,2 x 3,6 m" | object type "Curtain Wall:Fehr® Panneaux de Bardage 1,2 x 3,6 m:622585" | names: "Curtain Wall:Fehr® Panneaux de Bardage 1,2 x 3,6 m:621327", "Curtain Wall:Fehr® Panneaux de Bardage 1,2 x 3,6 m:648513" | parts: 113 IFCMEMBER, 56 IFCPLATE | property sets: Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Horizontal Grid, Other
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Fehr® Solution Panneaux de Bardage 1,2 x 1,2 m" | object type "Basic Wall:Fehr® Solution Panneaux de Bardage 1,2 x 1,2 m:623895" | names: "Basic Wall:Fehr® Solution Panneaux de Bardage 1,2 x 1,2 m:623894" | material: layers "Basic Wall:Fehr® Solution Panneaux de Bardage 1,2 x 1,2 m" ("Fehr® panneaux standard 1.2 x 1.2m" 16., "Air" 45., "Insulation" 120., "Concrete - Cast In Situ" 200.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | object type "Logo" | names: "Logo:Logo:626531" | material: materials ("Fehr® Logo Color Vert", "Fehr® Logo Color Gris") | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon, Constraints, Dimensions, Phasing
          1 x IFCANNOTATION

Types
  IFCWALLTYPE "Basic Wall:Fehr® Solution Panneaux de Bardage 1,2 x 2,4 m" | STANDARD | 1 occurrence | material: layers "Basic Wall:Fehr® Solution Panneaux de Bardage 1,2 x 2,4 m" ("Fehr® panneaux standard 1.2 x 2.4m" 16., "<Unnamed>" 45., "<Unnamed>" 120., "<Unnamed>" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:Ductal® Solution Panneaux de Bardage 1,2 x 3,6 m" | STANDARD | 1 occurrence | material: layers "Basic Wall:Ductal® Solution Panneaux de Bardage 1,2 x 3,6 m" ("Fehr® panneaux standard 1.2 x 3.6m" 16., "<Unnamed>" 45., "<Unnamed>" 120., "<Unnamed>" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:Fehr® Solution Panneaux de Bardage béton/isolant" | STANDARD | 5 occurrences | material: layers "Basic Wall:Fehr® Solution Panneaux de Bardage béton/isolant" ("Air" 45., "Insulation" 120., "Concrete - Cast In Situ" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCCURTAINWALLTYPE "Curtain Wall:Fehr® Panneaux de Bardage 1,2 x 1,2 m" | 1 occurrence | property sets: Construction, Horizontal Grid, Horizontal Mullions, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:Fehr® Panneaux de Bardage 1,2 x 2,4 m" | 2 occurrences | property sets: Construction, Horizontal Grid, Horizontal Mullions, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:Fehr® Panneaux de Bardage 1,2 x 3,6 m" | 2 occurrences | property sets: Construction, Horizontal Grid, Horizontal Mullions, Identity Data, Other, Vertical Grid
  IFCWALLTYPE "Basic Wall:Fehr® Solution Panneaux de Bardage 1,2 x 1,2 m" | STANDARD | 1 occurrence | material: layers "Basic Wall:Fehr® Solution Panneaux de Bardage 1,2 x 1,2 m" ("Fehr® panneaux standard 1.2 x 1.2m" 16., "Air" 45., "Insulation" 120., "Concrete - Cast In Situ" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other

Property sets
  Constraints | properties | on 548 objects (360 IFCMEMBER, 188 IFCPLATE)
    Level = "Level: Ductal Lafarge" (IFCLABEL)
  Constraints | properties | on 360 objects (360 IFCMEMBER)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 15 objects (15 IFCBUILDINGELEMENTPROXY)
    Work Plane = "Level : Ductal Lafarge" (IFCTEXT)
  Constraints | properties | on 6 objects (6 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Ductal Lafarge" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 8000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 3 objects (3 IFCCURTAINWALL)
    Base Constraint = "Level: Ductal Lafarge" (IFCLABEL)
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 8000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 2 objects (2 IFCCURTAINWALL)
    Base Constraint = "Level: Ductal Lafarge" (IFCLABEL)
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 8400. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Ductal Lafarge" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 8400. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints: 2 more contents on 2 objects not shown
  Dimensions | properties | on 360 objects (360 IFCMEMBER)
    Width on side 1 = 5. (IFCLENGTHMEASURE) [MILLI METRE]
    Width on side 2 = 5. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 119 objects (119 IFCMEMBER)
    Area = 0.0239000000000001 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 1190. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.000119 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 66 objects (66 IFCMEMBER)
    Area = 0.0241 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.00012 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 43 objects (43 IFCPLATE)
    Area = 1.41610000000001 (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 1190. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0226576000000001 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Width = 1190.00000000001 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 25 objects (25 IFCMEMBER)
    Area = 0.0163 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 810. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 8.10000000000000E-5 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 21 objects (21 IFCPLATE)
    Area = 0.957950000000005 (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 805. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0153272000000001 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Width = 1190.00000000001 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 20 objects (20 IFCMEMBER)
    Area = 0.0242 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 1205. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0001205 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 18 objects (18 IFCPLATE)
    Area = 2.8441 (IFCAREAMEASURE) [SQUARE_METRE]
    Height = 2390. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0455056 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Width = 1190. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions: 71 more contents on 266 objects not shown
  Other | properties | on 360 objects (360 IFCMEMBER)
    Category = "Curtain Wall Mullions" (IFCLABEL)
    Family Name = "Rectangular Mullion" (IFCTEXT)
  Other | properties | on 124 objects (124 IFCMEMBER)
    Category = "Curtain Wall Mullions" (IFCLABEL)
    Family = "Rectangular Mullion: Panel Border" (IFCLABEL)
    Family and Type = "Rectangular Mullion: Panel Border" (IFCLABEL)
    Host Id = "Curtain Wall: Fehr® Panneaux de Bardage 1,2 x 2,4 m" (IFCLABEL)
    Type = "Rectangular Mullion: Panel Border" (IFCLABEL)
    Type Id = "Rectangular Mullion: Panel Border" (IFCLABEL)
  Other | properties | on 123 objects (123 IFCMEMBER)
    Category = "Curtain Wall Mullions" (IFCLABEL)
    Family = "Rectangular Mullion: Panel Border" (IFCLABEL)
    Family and Type = "Rectangular Mullion: Panel Border" (IFCLABEL)
    Host Id = "Curtain Wall: Fehr® Panneaux de Bardage 1,2 x 1,2 m" (IFCLABEL)
    Type = "Rectangular Mullion: Panel Border" (IFCLABEL)
    Type Id = "Rectangular Mullion: Panel Border" (IFCLABEL)
  Other | properties | on 113 objects (113 IFCMEMBER)
    Category = "Curtain Wall Mullions" (IFCLABEL)
    Family = "Rectangular Mullion: Panel Border" (IFCLABEL)
    Family and Type = "Rectangular Mullion: Panel Border" (IFCLABEL)
    Host Id = "Curtain Wall: Fehr® Panneaux de Bardage 1,2 x 3,6 m" (IFCLABEL)
    Type = "Rectangular Mullion: Panel Border" (IFCLABEL)
    Type Id = "Rectangular Mullion: Panel Border" (IFCLABEL)
  Other | properties | on 70 objects (70 IFCPLATE)
    Category = "Curtain Panels" (IFCLABEL)
    Family = "System Panel: Fehr® Panneaux de Bardage" (IFCLABEL)
    Family and Type = "System Panel: Fehr® Panneaux de Bardage" (IFCLABEL)
    Host Id = "Curtain Wall: Fehr® Panneaux de Bardage 1,2 x 1,2 m" (IFCLABEL)
    Type = "System Panel: Fehr® Panneaux de Bardage" (IFCLABEL)
    Type Id = "System Panel: Fehr® Panneaux de Bardage" (IFCLABEL)
  Other | properties | on 62 objects (62 IFCPLATE)
    Category = "Curtain Panels" (IFCLABEL)
    Family = "System Panel: Fehr® Panneaux de Bardage" (IFCLABEL)
    Family and Type = "System Panel: Fehr® Panneaux de Bardage" (IFCLABEL)
    Host Id = "Curtain Wall: Fehr® Panneaux de Bardage 1,2 x 2,4 m" (IFCLABEL)
    Type = "System Panel: Fehr® Panneaux de Bardage" (IFCLABEL)
    Type Id = "System Panel: Fehr® Panneaux de Bardage" (IFCLABEL)
  Other | properties | on 56 objects (56 IFCPLATE)
    Category = "Curtain Panels" (IFCLABEL)
    Family = "System Panel: Fehr® Panneaux de Bardage" (IFCLABEL)
    Family and Type = "System Panel: Fehr® Panneaux de Bardage" (IFCLABEL)
    Host Id = "Curtain Wall: Fehr® Panneaux de Bardage 1,2 x 3,6 m" (IFCLABEL)
    Type = "System Panel: Fehr® Panneaux de Bardage" (IFCLABEL)
    Type Id = "System Panel: Fehr® Panneaux de Bardage" (IFCLABEL)
  Other | properties | on 15 objects (15 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family Name = "Model Text" (IFCTEXT)
  Other: 16 more contents on 34 objects not shown
  Phasing | properties | on 577 objects (360 IFCMEMBER, 188 IFCPLATE, 16 IFCBUILDINGELEMENTPROXY, 8 IFCWALLSTANDARDCASE)
    Phase Created = "New Construction" (IFCLABEL)
  Structural | properties | on 13 objects (8 IFCWALLSTANDARDCASE, 5 IFCCURTAINWALL)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 5 objects (5 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "M0 (classification française)" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Fehr® Solution Panneaux de Bardage béton/isolant" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "M0 (classification française)" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Fehr® Solution Panneaux de Bardage 1,2 x 2,4 m" (IFCIDENTIFIER)
    ThermalTransmittance = 153.125 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "M0 (classification française)" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Ductal® Solution Panneaux de Bardage 1,2 x 3,6 m" (IFCIDENTIFIER)
    ThermalTransmittance = 153.125 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "M0 (classification française)" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Fehr® Solution Panneaux de Bardage 1,2 x 1,2 m" (IFCIDENTIFIER)
    ThermalTransmittance = 153.125 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_ManufacturerTypeInformation | properties | on 201 objects (188 IFCPLATE, 8 IFCWALLSTANDARDCASE, 5 IFCCURTAINWALL)
    Manufacturer = "Fehr®" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 8 objects (8 IFCBUILDINGELEMENTPROXY)
    Reference = "600mm Arial" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 7 objects (7 IFCBUILDINGELEMENTPROXY)
    Reference = "300mm Arial" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Logo" (IFCIDENTIFIER)
  Graphics | properties | on 7 objects (7 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "®" (IFCTEXT)
  Graphics | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "Fehr Panneaux de Bardage 1,2 x 2,4 m Niveau de détail élevé" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "Fehr Panneaux de Bardage 1,2 x 3,6 m Niveau de détail élevé" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "Fehr Panneaux de Bardage 1,2 x 1,2 m Niveau de détail élevé" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "Fehr Panneaux de Bardage 1,2 x 3,6 m Niveau de détail basique" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "Fehr Panneaux de Bardage 1,2 x 2,4 m Niveau de détail basique" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Horizontal Align = "Left" (IFCIDENTIFIER)
    Text = "Fehr Panneaux de Bardage 1,2 x 1,2 m Niveau de détail basique" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Graphics: 2 more contents on 1 objects not shown
  Identity Data | properties | on 360 objects (360 IFCMEMBER)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "Panel Border" (IFCTEXT)
  Identity Data | properties | on 15 objects (15 IFCBUILDINGELEMENTPROXY)
    Subcategory = "Generic Models" (IFCLABEL)
  Identity Data | properties | on 8 objects (8 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "600mm Arial" (IFCTEXT)
  Identity Data | properties | on 7 objects (7 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "300mm Arial" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "Logo" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Ductal Lafarge" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data: 7 more contents on 0 objects not shown
  Materials and Finishes | properties | on 360 objects (360 IFCMEMBER)
    Material = "Joints et raccords de panneaux" (IFCLABEL)
  Materials and Finishes | properties | on 2 type objects
    Structural Material = "Concrete - Cast In Situ" (IFCLABEL)
  Construction | properties | on 360 objects (360 IFCMEMBER)
    Corner Mullion = FALSE (IFCBOOLEAN)
    Position = "Perpendicular to Face" (IFCLABEL)
    Profile = "Panel Distance: Panel Distance" (IFCLABEL)
    Thickness = 10. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 3 type objects
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 381. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 3 type objects
    Automatically Embed = FALSE (IFCBOOLEAN)
    Curtain Panel = "System Panel: Fehr® Panneaux de Bardage" (IFCLABEL)
    Function = "Exterior" (IFCIDENTIFIER)
    Join Condition = "Not Defined" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 365. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Text | properties | on 8 objects (8 IFCBUILDINGELEMENTPROXY)
    Bold = FALSE (IFCBOOLEAN)
    Italic = FALSE (IFCBOOLEAN)
    Text Font = "Arial" (IFCTEXT)
    Text Size = 600. (IFCLENGTHMEASURE) [MILLI METRE]
  Text | properties | on 7 objects (7 IFCBUILDINGELEMENTPROXY)
    Bold = FALSE (IFCBOOLEAN)
    Italic = FALSE (IFCBOOLEAN)
    Text Font = "Arial" (IFCTEXT)
    Text Size = 300. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Vertical Grid | properties | on 2 objects (2 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 7 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid | properties | on 2 objects (2 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 8 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid | properties | on 1 object (1 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 9 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid | properties | on 3 type objects
    Adjust for Mullion Size = TRUE (IFCBOOLEAN)
    Layout = "Fixed Distance" (IFCIDENTIFIER)
    Spacing = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
  Horizontal Grid | properties | on 2 objects (2 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 2 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Horizontal Grid | properties | on 2 objects (2 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 3 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Horizontal Grid | properties | on 1 object (1 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 6 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Horizontal Grid | properties | on 1 type object
    Adjust for Mullion Size = TRUE (IFCBOOLEAN)
    Layout = "Fixed Distance" (IFCIDENTIFIER)
    Spacing = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
  Horizontal Grid | properties | on 1 type object
    Adjust for Mullion Size = TRUE (IFCBOOLEAN)
    Layout = "Fixed Distance" (IFCIDENTIFIER)
    Spacing = 2400. (IFCLENGTHMEASURE) [MILLI METRE]
  Horizontal Grid | properties | on 1 type object
    Adjust for Mullion Size = TRUE (IFCBOOLEAN)
    Layout = "Fixed Distance" (IFCIDENTIFIER)
    Spacing = 3600. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 134 objects (134 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Panel Border" (IFCIDENTIFIER)
    Span = 1190. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 66 objects (66 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Panel Border" (IFCIDENTIFIER)
    Span = 1200. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 25 objects (25 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Panel Border" (IFCIDENTIFIER)
    Span = 810. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 20 objects (20 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Panel Border" (IFCIDENTIFIER)
    Span = 1205. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 18 objects (18 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Panel Border" (IFCIDENTIFIER)
    Span = 2400. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 17 objects (17 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Panel Border" (IFCIDENTIFIER)
    Span = 1197.5 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 14 objects (14 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Panel Border" (IFCIDENTIFIER)
    Span = 1195. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 11 objects (11 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Panel Border" (IFCIDENTIFIER)
    Span = 1185. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon: 12 more contents on 55 objects not shown
  Pset_CurtainWallCommon | properties | on 2 objects (2 IFCCURTAINWALL)
    FireRating = "M0 (classification française), A2s1d0 ( classification européenne)" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Fehr® Panneaux de Bardage 1,2 x 2,4 m" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 2 objects (2 IFCCURTAINWALL)
    FireRating = "M0 (classification française), A2s1d0 ( classification européenne)" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Fehr® Panneaux de Bardage 1,2 x 3,6 m" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    FireRating = "M0 (classification française), A2s1d0 ( classification européenne)" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Fehr® Panneaux de Bardage 1,2 x 1,2 m" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 188 objects (188 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Fehr® Panneaux de Bardage" (IFCIDENTIFIER)
  Analytical Properties | properties | on 3 type objects
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 153.125 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 0.00653061224489796 (IFCREAL)
    Thermal mass = 34224. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
  Horizontal Mullions | properties | on 3 type objects
    Interior Type = "Rectangular Mullion: Panel Border" (IFCLABEL)
  Vertical Mullions | properties | on 3 type objects
    Interior Type = "Rectangular Mullion: Panel Border" (IFCLABEL)