IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2016-12-16T15:21:38"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20140223_1515(x64) - Exporter 2015.0.2014.0223 - Default UI"
Application: "Autodesk Revit 2015 (FRA)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (FRA)"

People and organizations
  Person "ywy" of Organization (no name given)
  Owner history of Person "ywy" of Organization (no name given) | application "Autodesk Revit 2015 (FRA)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (FRA)" | change NOCHANGE | created 1481783574 (2016-12-15T06:32:54Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Fehr" | long name "Fehr" | elevation 0.
        contains 8 elements
          1 x IFCBUILDINGELEMENTPROXY | object type "模型文字:600mm Arial" | names: "模型文字:600mm Arial" | property sets: Pset_BuildingElementProxyCommon, 其他, 图形, 尺寸标注, 材质和装饰, 标识数据
          2 x IFCBUILDINGELEMENTPROXY | object type "模型文字:300mm Arial" | names: "模型文字:300mm Arial" | property sets: Pset_BuildingElementProxyCommon, 其他, 图形, 尺寸标注, 标识数据, 阶段化
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "基本墙:Fehr® Mur Précoffré® Classique" | object type "基本墙:Fehr® Mur Précoffré® Classique:414954" | names: "基本墙:Fehr® Mur Précoffré® Classique:623894", "基本墙:Fehr® Mur Précoffré® Classique:939023", "基本墙:Fehr® Mur Précoffré® Classique:939024" | material: layers "基本墙:Fehr® Mur Précoffré® Classique" ("FEHR® PEAU EXTERIEURE LISSE" 55., "FEHR® NOYAU A COULER EN PLACE" 90., "FEHR® PEAU INTERIEURE LISSE" 55.) | property sets: 其他, 尺寸标注, 结构, 阶段化, 限制条件, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | object type "Logo" | names: "Logo:Logo:626531" | material: materials ("Fehr® Logo Color Vert", "Fehr® Logo Color Gris") | property sets: Pset_BuildingElementProxyCommon, 其他, 尺寸标注, 阶段化, 限制条件, 标识数据
          1 x IFCBUILDINGELEMENTPROXY | object type "模型文字:600mm Arial 2" | names: "模型文字:600mm Arial 2" | property sets: Pset_BuildingElementProxyCommon, 其他, 图形, 尺寸标注, 材质和装饰, 标识数据

Types
  IFCWALLTYPE "基本墙:Fehr® Mur Précoffré® Classique" | STANDARD | 3 occurrences | material: layers "基本墙:Fehr® Mur Précoffré® Classique" ("FEHR® PEAU EXTERIEURE LISSE" 55., "FEHR® NOYAU A COULER EN PLACE" 90., "FEHR® PEAU INTERIEURE LISSE" 55.) | property sets: 其他, 分析属性, 图形, 材质和装饰, 构造, 标识数据

Property sets
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "300mm Arial" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "600mm Arial" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Logo" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "600mm Arial 2" (IFCIDENTIFIER)
  其他 | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    族名称 = "模型文字" (IFCTEXT)
    类别 = "常规模型" (IFCLABEL)
  其他 | properties | on 3 objects (3 IFCWALLSTANDARDCASE)
    族 = "基本墙: Fehr® Mur Précoffré® Classique" (IFCLABEL)
    族与类型 = "基本墙: Fehr® Mur Précoffré® Classique" (IFCLABEL)
    类别 = "墙" (IFCLABEL)
    类型 = "基本墙: Fehr® Mur Précoffré® Classique" (IFCLABEL)
    类型 ID = "基本墙: Fehr® Mur Précoffré® Classique" (IFCLABEL)
  其他 | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    族 = "模型文字: 300mm Arial" (IFCLABEL)
    族与类型 = "模型文字: 300mm Arial" (IFCLABEL)
    类别 = "常规模型" (IFCLABEL)
    类型 = "模型文字: 300mm Arial" (IFCLABEL)
    类型 ID = "模型文字: 300mm Arial" (IFCLABEL)
  其他 | properties | on 2 objects (2 IFCOPENINGELEMENT)
    主体 ID = "基本墙: Fehr® Mur Précoffré® Classique" (IFCLABEL)
    族 = "Joint Angle 90°: Joint Angle 90°" (IFCLABEL)
    族与类型 = "Joint Angle 90°: Joint Angle 90°" (IFCLABEL)
    类别 = "结构连接" (IFCLABEL)
    类型 = "Joint Angle 90°: Joint Angle 90°" (IFCLABEL)
    类型 ID = "Joint Angle 90°: Joint Angle 90°" (IFCLABEL)
  其他 | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    客户姓名 = "Owner" (IFCTEXT)
    类别 = "项目信息" (IFCLABEL)
    项目发布日期 = "Issue Date" (IFCTEXT)
    项目名称 = "Project Name" (IFCTEXT)
    项目地址 = "Enter address here" (IFCTEXT)
    项目状态 = "Project Status" (IFCTEXT)
    项目编号 = "Project Number" (IFCTEXT)
  其他 | properties | on 2 objects (2 IFCOPENINGELEMENT)
    族名称 = "Joint Angle 90°" (IFCTEXT)
    类别 = "结构连接" (IFCLABEL)
  其他 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    族 = "模型文字: 600mm Arial" (IFCLABEL)
    族与类型 = "模型文字: 600mm Arial" (IFCLABEL)
    类别 = "常规模型" (IFCLABEL)
    类型 = "模型文字: 600mm Arial" (IFCLABEL)
    类型 ID = "模型文字: 600mm Arial" (IFCLABEL)
  其他 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    族 = "Logo: Logo" (IFCLABEL)
    族与类型 = "Logo: Logo" (IFCLABEL)
    类别 = "常规模型" (IFCLABEL)
    类型 = "Logo: Logo" (IFCLABEL)
    类型 ID = "Logo: Logo" (IFCLABEL)
  其他: 9 more contents on 8 objects not shown
  图形 | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    文字 = "®" (IFCTEXT)
    水平对齐 = "左" (IFCIDENTIFIER)
  图形 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    文字 = "Fehr Mur Précoffré Classique" (IFCTEXT)
    水平对齐 = "左" (IFCIDENTIFIER)
  图形 | properties | on 1 object (1 IFCBUILDINGSTOREY)
    端点 1 处的默认符号 = FALSE (IFCBOOLEAN)
    端点 2 处的默认符号 = TRUE (IFCBOOLEAN)
    符号 = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    线型图案 = "Centre" (IFCLABEL)
    线宽 = "1" (IFCIDENTIFIER)
    颜色 = 0 (IFCINTEGER)
  图形 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    文字 = "Joint d'angle 90° Faux joint Joint droit" (IFCTEXT)
    水平对齐 = "左" (IFCIDENTIFIER)
  图形 | properties | on 1 type object
    粗略比例填充颜色 = 0 (IFCINTEGER)
  尺寸标注 | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    深度 = 10. (IFCLENGTHMEASURE) [MILLI METRE]
  尺寸标注 | properties | on 2 objects (2 IFCOPENINGELEMENT)
    Epaisseur Joint = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Epaisseur Mur = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Epaisseur Peau Interieure = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    Epaisseur Peau exterieure = 55. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur Joint = 8000. (IFCLENGTHMEASURE) [MILLI METRE]
    Information Utilisation Objet Joint = "Mettre dans l'objet "joint" les mêmes valeurs de parametres que dans le mur corespondant." (IFCTEXT)
    Longueur Joint = 165. (IFCLENGTHMEASURE) [MILLI METRE]
  尺寸标注 | properties | on 2 objects (2 IFCOPENINGELEMENT)
    Ouverture Front = 30. (IFCLENGTHMEASURE) [MILLI METRE]
  尺寸标注 | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    体积 = 16. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    长度 = 10000. (IFCLENGTHMEASURE) [MILLI METRE]
    面积 = 80.0000000000001 (IFCAREAMEASURE) [SQUARE_METRE]
  尺寸标注 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    体积 = 0.143947226058033 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    面积 = 4.43022169733772 (IFCAREAMEASURE) [SQUARE_METRE]
  尺寸标注 | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    体积 = 14.7068 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    长度 = 9200.00000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    面积 = 73.8400000000159 (IFCAREAMEASURE) [SQUARE_METRE]
  尺寸标注 | properties | on 1 object (1 IFCOPENINGELEMENT)
    Epaisseur Joint = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur Joint = 8000. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur Joint = 40.0000000000005 (IFCLENGTHMEASURE) [MILLI METRE]
    Profondeur Joint = 10.0000000000002 (IFCLENGTHMEASURE) [MILLI METRE]
  尺寸标注 | properties | on 1 object (1 IFCOPENINGELEMENT)
    Hauteur Joint = 8000. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur Joint = 40.0000000000005 (IFCLENGTHMEASURE) [MILLI METRE]
    Profondeur Joint = 10.0000000000002 (IFCLENGTHMEASURE) [MILLI METRE]
  尺寸标注: 3 more contents on 3 objects not shown
  材质和装饰 | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    材质 = "Fehr® Logo Color Gris" (IFCLABEL)
  材质和装饰 | properties | on 1 type object
    结构材质 = "FEHR® NOYAU A COULER EN PLACE" (IFCLABEL)
  标识数据 | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    子类别 = "常规模型" (IFCLABEL)
  标识数据 | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    作者 = "" (IFCTEXT)
    建筑名称 = "" (IFCTEXT)
    组织名称 = "" (IFCTEXT)
    组织描述 = "" (IFCTEXT)
  标识数据 | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    类型名称 = "300mm Arial" (IFCTEXT)
    部件代码 = "" (IFCTEXT)
    部件说明 = "" (IFCTEXT)
  标识数据 | properties | on 2 objects (2 IFCOPENINGELEMENT)
    OmniClass 标题 = "" (IFCTEXT)
    OmniClass 编号 = "" (IFCTEXT)
    类型名称 = "Joint Angle 90°" (IFCTEXT)
    部件代码 = "" (IFCTEXT)
    部件说明 = "" (IFCTEXT)
  标识数据 | properties | on 1 object (1 IFCBUILDINGSTOREY)
    类型名称 = "8mm Head" (IFCTEXT)
  标识数据 | properties | on 1 object (1 IFCBUILDINGSTOREY)
    名称 = "Fehr" (IFCTEXT)
    建筑楼层 = TRUE (IFCBOOLEAN)
    结构 = FALSE (IFCBOOLEAN)
  标识数据 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    类型名称 = "600mm Arial" (IFCTEXT)
    部件代码 = "" (IFCTEXT)
    部件说明 = "" (IFCTEXT)
  标识数据 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    OmniClass 标题 = "" (IFCTEXT)
    OmniClass 编号 = "" (IFCTEXT)
    类型名称 = "Logo" (IFCTEXT)
    部件代码 = "" (IFCTEXT)
    部件说明 = "" (IFCTEXT)
  标识数据: 4 more contents on 3 objects not shown
  阶段化 | properties | on 12 objects (5 IFCBUILDINGELEMENTPROXY, 4 IFCOPENINGELEMENT, 3 IFCWALLSTANDARDCASE)
    创建的阶段 = "New Construction" (IFCLABEL)
  限制条件 | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    工作平面 = "标高 : Fehr" (IFCTEXT)
  限制条件 | properties | on 4 objects (4 IFCOPENINGELEMENT)
    标高 = "标高: Fehr" (IFCLABEL)
    立面 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  限制条件 | properties | on 3 objects (3 IFCWALLSTANDARDCASE)
    与体量相关 = FALSE (IFCBOOLEAN)
    定位线 = "墙中心线" (IFCIDENTIFIER)
    已附着底部 = FALSE (IFCBOOLEAN)
    已附着顶部 = FALSE (IFCBOOLEAN)
    底部偏移 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    底部延伸距离 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    底部限制条件 = "标高: Fehr" (IFCLABEL)
    房间边界 = TRUE (IFCBOOLEAN)
    无连接高度 = 8000. (IFCLENGTHMEASURE) [MILLI METRE]
    顶部偏移 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    顶部延伸距离 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  限制条件 | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    与邻近图元一同移动 = FALSE (IFCBOOLEAN)
    主体 = "标高 : Fehr" (IFCTEXT)
    偏移量 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    标高 = "标高: Fehr" (IFCLABEL)
  限制条件 | properties | on 1 object (1 IFCBUILDINGSTOREY)
    基面 = "项目基点" (IFCIDENTIFIER)
  限制条件 | properties | on 1 object (1 IFCBUILDINGSTOREY)
    立面 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  结构 | properties | on 3 objects (3 IFCWALLSTANDARDCASE)
    启用分析模型 = FALSE (IFCBOOLEAN)
    结构 = FALSE (IFCBOOLEAN)
    结构用途 = "非承重" (IFCIDENTIFIER)
  结构 | properties | on 2 objects (2 IFCOPENINGELEMENT)
    钢筋保护层 = "钢筋保护层设置: Rebar Cover 1" (IFCLABEL)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "M0 (classification française)" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Fehr® Mur Précoffré® Classique" (IFCIDENTIFIER)
    ThermalTransmittance = 9.50909090909091 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_ManufacturerTypeInformation | properties | on 7 objects (4 IFCOPENINGELEMENT, 3 IFCWALLSTANDARDCASE)
    Manufacturer = "Fehr" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  文字 | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    文字大小 = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    文字字体 = "Arial" (IFCTEXT)
    斜体 = FALSE (IFCBOOLEAN)
    粗体 = FALSE (IFCBOOLEAN)
  文字 | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    文字大小 = 165. (IFCLENGTHMEASURE) [MILLI METRE]
    文字字体 = "Arial" (IFCTEXT)
    斜体 = FALSE (IFCBOOLEAN)
    粗体 = FALSE (IFCBOOLEAN)
  分析属性 | properties | on 1 type object
    传热系数(U) = 9.50909090909091 (IFCREAL)
    吸收率 = 0.1 (IFCREAL)
    热质量 = 166221. (IFCREAL)
    热阻(R) = 0.105162523900574 (IFCREAL)
    粗糙度 = 1 (IFCINTEGER)
  构造 | properties | on 1 type object
    功能 = "外部" (IFCIDENTIFIER)
    厚度 = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    在插入点包络 = "不包络" (IFCIDENTIFIER)
    在端点包络 = "无" (IFCIDENTIFIER)